                        Marked Points


The following is a list of current marked points:

999 center line  (pave)

1 top outside edge of pavement (pave)
2 bottom of outside edge of pavement (pave)

9 edge of traveled lane (pave)

43  marks "clear zone in dgn"    (tieslope&ditches)
47  marks "Match line in dgn"   (tieslope&ditches)

96,97 shoulder pi, or pi   (shoulder, berm, prerequisite for tieslope or ditch)

98,99 temporary, within a code

Criteria ranges

1-9             Pavement Points
10-25   Curb and gutter points, 21-25 tie-in points raised medians
26-34   Shoulder paved, composite and aggregate points
         Note: Point 3 is now Point 26
35-49   Ditches, tieslopes
50-60   Depressed Medians
90-100  Subsurface tie-ins, berms, sidewalks, shoulder pi's 
                 Note: Point 5 is now Point 90

100-149     Walls - Noise and retaining
150-175     Median Barrier Points
176-199     Wall adjuncts
200-225     Ponds
260-269     Shoulder Points
300-325     Inplace removal points
326-349     Waste and Disposal
400-420     Snow drift
600-630     Grading grade points
631-650     Base aggregate points, bit base
675-700     Select Granular Points
700-750     Subcut points
800-849     Shadow Points
900-950     User defined points



